Implement the idea of Translation look aside buffer. You can choose the TLB size to be 10. Also compute the Effective memory access time. Recall that the overall effective memory time was computed using the following expression:

**EMAT = h\*(CH+MM) + (1-h)\*(CH+2MM)**

MM= Main memory access time

CH= Cache access time